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МУАССИСАИ ДАВЛАТИИ СОХТМОНИ АСОСЇ ВА МЕЛИОРАТИВИИ
АГЕНТИИ БЕЊДОШТИ ЗАМИН ВА ОБЁРИИ НАЗДИ ЊУКУМАТИ
ЉУМЊУРИИ  ТОЉИКИСТОН
	
ш. Душанбе, кўчаи  Шамсї 5/1, тел./факс 235-15-83



Invitation for Bids 

Date: 17 August 2026

[bookmark: _Hlk133314550]Loan/Grant No. and Title: 0810TAJ(SF) / Climate- and Disaster-Resilient Irrigation and Drainage Modernization in the Vakhsh River Basin Project

Contract No. and Title: GDS-4 / Procurement of hose irrigation system and equipment: (Lot-1 Procurement of tools and farm equipment for mardikor groups and Lot-2 Procurement of (i) Hose and simple irrigation systems for Homestead Areas, and (ii) Gated pipes for farms)

Deadline for Submission of Bids: 15 September 2026


1. The Republic of Tajikistan has received financing from the Asian Development Bank (ADB) toward the cost of Climate- and Disaster-Resilient Irrigation and Drainage Modernization in the Vakhsh River Basin Project, and it intends to apply part of the proceeds of this financing to payments under the contract named above. Bidding is open to Bidders from eligible source countries of ADB.

2. [bookmark: _GoBack]The Agency for Land Reclamation and Irrigation (ALRI) (“the Purchaser”) invites sealed bids from eligible Bidders for GDS-4 / Procurement of hose irrigation system and equipment: (Lot-1 Procurement of tools and farm equipment for mardikor groups and Lot-2 Procurement of (i) Hose and simple irrigation systems for Homestead Areas, and (ii) Gated pipes for farms). The list of equipment, delivery period and location as follow:

	No:
	Item
	Quantity
	Delivery time
	Location

	Lot-1 Procurement of tools and farm equipment for mardikor groups

	1
	Motoblock
	4
	3 months
	Republic of Tajikistan, Shamsi Str 5/1, Dushanbe, Tajikistan 

	2
	Cargo scooter
	4
	
	

	3
	Mini tractor
	4
	
	

	4
	Sprayer
	8
	
	

	5
	Garden cart
	8
	
	

	6
	Scoop shovel
	100
	
	

	7
	Bayonet shovel
	100
	
	

	8
	Ketmen
	100
	
	

	9
	Garden pitchfork
	100
	
	

	10
	Rake
	50
	
	

	11
	Hoe
	50
	
	

	12
	Sickle
	200
	
	

	13
	Construction gloves
	1000
	
	

	14
	Masks (medical)
	5000
	
	

	15
	Women's work robe size M
	50
	
	

	16
	Women's work robe size L
	75
	
	

	17
	Women's work robe size XL
	75
	
	

	18
	Cotton collecting bag
	200
	
	

	19
	Rubber boots size 39
	100
	
	

	20
	Rubber boots, size 40
	100
	
	

	21
	Protective cap
	300
	
	

	22
	Umbrella for shelter on the field
	20
	
	

	23
	Garden shears (pruning shears)
	80
	
	

	24
	Hacksaw By tree
	100
	
	

	25
	Hacksaw By metal
	100
	
	

	26
	Taiga axe
	100
	
	

	27
	Overalls for working with chemicals
	20
	
	

	28
	Film layer 
	8
	
	

	29
	Reflective safety vest for workers (size M )
	50
	
	

	30
	Reflective safety vest for workers (size L )
	100
	
	

	31
	Reflective safety vest for workers (size XL )
	100
	
	

	Lot-2 Procurement of (i) Hose and simple irrigation systems for Homestead Areas, and (ii) Gated pipes for farms

	1
	Polyethylene pipe Ø = 160 x 7.7 mm PE 100, SDR 21, PN8
	6376
	3 months
	Republic of Tajikistan, Shamsi Str 5/1, Dushanbe, Tajikistan 

	2
	Polyethylene pipe Ø = 75 x 3.6 mm PE 100, SDR 21, PN8
	12444
	
	

	3
	Polyethylene pipe Ø = 50 x 2.4 mm PE 100, SDR 21, PN8
	10600
	
	

	4
	Polyethylene pipe Ø = 110 x 5.3 mm PE 100, SDR 21, PN8
	8944
	
	

	5
	Polyethylene pipe Ø = 225 x 10.8 mm PE 100, SDR 21, PN8
	340
	
	

	6
	PPR pipe Ø = 32 mm L = 1600 mm
	250
	
	

	7
	Cast transition tee Ø = 160 x 50 mm PE 100, SDR 11
	35
	
	

	8
	Cast transition tee Ø = 75 x 50 mm PE 100, SDR 11
	11
	
	

	9
	Cast transition tee Ø = 160 x 75 mm PE 100, SDR 11
	1
	
	

	10
	Cast transition tee Ø = 160 x 110 mm PE 100, SDR 11
	7
	
	

	11
	Cast transition tee Ø = 110 x 75 mm PE 100, SDR 11
	7
	
	

	12
	Cast reducing tee Ø = 110 x 32 mm PE 100, SDR 11
	17
	
	

	13
	Cast reducing tee Ø = 75 x 32 mm PE 100, SDR 11
	84
	
	

	14
	Cast reducing tee Ø = 50 x 32 mm PE 100, SDR 11
	108
	
	

	15
	Cast reducing tee Ø = 160 x 32 mm PE 100, SDR 11
	19
	
	

	16
	Gate valve Ø = 150 mm L = 280 mm 30С42NJ
	3
	
	

	17
	Gate valve Ø = 100 mm L = 280 mm 30С42NJ
	3
	
	

	18
	Gate valve Ø = 65 mm L = 190 mm 15KCH18P
	1
	
	

	19
	Steel ring flange Ø = 100 – 160mm, PN= 10.0 kg/cm2
	12
	
	

	20
	Flange bushing Ø = 100 – 160mm, PN= 10.0 kg/cm2
	12
	
	

	21
	Plastic valve PPR Ø = 32 mm
	190
	
	

	22
	Elbow 90 degrees PPR Ø = 32 mm
	456
	
	



3.	Open competitive bidding will be conducted in accordance with ADB’s Single-Stage: One-Envelope Bidding Procedure Without Prequalification, without Merit Point Criteria (MPC) procedure and is open to all Bidders from eligible countries as described in the Bidding Document.

4.	Only eligible Bidders with the following key qualifications defined in the Bidding Document may participate in this bidding:
	a) Historical Financial Performance
	Submission of audited financial statements or, if not required by the law of the Bidder’s country, other financial statements acceptable to the Purchaser, for the last three (3) years to demonstrate the current soundness of the Bidder’s financial position. As a minimum, the Bidder’s net worth for the last year calculated as the difference between total assets and total liabilities should be positive.

	c) Average Annual Turnover
	Minimum average annual turnover 
Lot-1: USD 212,400.00
Lot-2: USD 842,520.00
calculated as total payments received by the Bidder for contracts completed or under execution over the last three (3) years.
Minimum average annual turnover of Bids for multiple Lots shall be the aggregate sum of the turnover for individual Lots (Lot 1 and Lot 2) calculated as total payments received by the Bidder for contracts completed or under execution over the last (3) years.

	d) Contractual Experience
	Successful completion as main supplier within the last three (3) years, of at least two (2) contracts each valued at 
Lot-1: USD 84,960.00
Lot-2: USD 337,008.00 
with nature, and complexity similar to the scope of supply described in Section 6 (Schedule of Supply).
Minimum value for contracts of Bids for multiple Lots shall be the aggregate sum of the individual Lots (Lot 1 and Lot 2) with nature, and complexity similar to the scope of supply described in Section 6 (Schedule of Supply)




5.	To obtain further information and inspect the Bidding Documents, Bidders should contact: 

Project Implementation Group (PIG) under the
SI "Capital and Land Reclamation Construction" under ALRI
734064, Shamsi street 5/1, Dushanbe City Republic of Tajikistan
Contact Person: Mr. Farhod Abdullozoda
E-mail: alri_project@mail.ru
	

6.	To obtain the Bidding Documents in English, eligible Bidders should
· write to the address above requesting the Bidding Documents for GDS-4 / Procurement of hose irrigation system and equipment: (Lot-1 Procurement of tools and farm equipment for mardikor groups and Lot-2 Procurement of (i) Hose and simple irrigation systems for Homestead Areas, and (ii) Gated pipes for farms).


The document will be sent in PDF format via email. 

7.	Deliver your bid:
· to the address:
State Committee for Investments and State Property Management of the Republic of Tajikistan
Street address: Rudaki avenue 40
Floor/Room number: 2nd floor, Tender Room 
City: Dushanbe
ZIP code: 734000
Country: Republic of Tajikistan
 
· on or before the deadline: 15 September 2026, 14:00 hrs. (Dushanbe local time) and
· together with a Bid Security as described in the Bidding Document.

	Bids will be opened promptly after the deadline for bid submission in the presence of Bidders’ representatives who choose to attend. 



INTERNAL. This information is accessible to ADB Management and Staff. It may be shared outside ADB with appropriate permission.
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